Ghana

National Policy

Operator Licensing

Technical and Administrative Requirements

Licensing Fees

Access to Spectrum

Technical and Administrative Requirements

Licensed

Access Networks

Operator	700 MHz	800 MHz	900 MHz	1800 MHz	2100 MHz	2300 MHz	2600 MHz	3500MHz
AirtelTigo	2X13	2X10	2X10
Blu Telecommunications	30
Busy	30
Glo	2X5	2X15	2X10
Goldkey	2X15
MTN	2X10	2X8	2X10	2X15	2X15
Surfline	2X15
Telesol
Tigo	2X8	2X10	2X15
Vodafone	2X5	2X8	2X10	2X15

PtP Networks

License-Exempt

Access Networks

Frequency	Power Limit	Transmit Power
2.4GHz
2400 – 2483.5 MHz	2.4EIRP
5GHz
5150-5250 MHz	5.1EIRP
5250-5350 MHz	5.2EIRP
5470-5725 MHz	5.4EIRP
5725-5800 MHz	5.8EIRP

PtP Networks

Frequency	Power Limit	Transmit Power
2.4GHz
2400 – 2483.5 MHz	2.4EIRP
5GHz
5150-5250 MHz	5.1EIRP
5250-5350 MHz	5.2EIRP
5470-5725 MHz	5.4EIRP
5725-5800 MHz	5.8EIRP

Secondary Use

Access Networks

PtP Networks

Spectrum Fees / Costs

Application

Annual

Auction

Backhaul

Gender

Universal Service

Cooperatives

Resources / References

Coding examples

This could be used to frame specific questions that should be asked

<callout type=“tip” icon=“true”>This could be for hints / tips / tricks on finding information, what to look for etc.</callout> <callout type=“question” icon=“true”>A question</callout> <callout type=“success” icon=“true”>A good practice example might look like this</callout> <callout type=“danger” icon=“true”>A bad practice to be aware of might look like this</callout>